Lakeview School District
Elementary Digital Sign Replacement Project
SECTION 1
Procurement & Contracting Requirements

Advertisement for Bids
Lakeview School District invites sealed bids for the furnishing of all labor, materials, equipment, supervision, permits, engineering, demolition, construction, electrical coordination, installation, testing, startup, training, warranty service, and related work necessary to replace existing monument signs with new digital monument signs at Minges Brook, Prairieview, Riverside, and Westlake Elementary Schools.

The Board of Education reserves the right to reject any or all bids, waive informalities, and award the project in whole or by individual school as determined to be in the best interest of the District.
Instructions to Bidders
Purpose
Provide a complete turnkey digital monument sign replacement project.
Questions
Submit all questions in writing to:
	Laura McFadden
	Todd Pullano

	Assistant Superintendent of Finance
	Director of Operations

	lmcfadden@lakeviewspartans.org
	tpullano@lakeviewspartans.org


Bid Security
Bid Security in the form of a certified check for 5% of the bid payable to Lakeview School District is acceptable bid security only for proposals less than $50,000. Bid Security in the form of bonds is required to be submitted with all proposals greater than $50,000. 
Insurance
       Provide Commercial General Liability, Automobile Liability, Workers Compensation, Employer's Liability, and             Umbrella coverage naming Lakeview School District as Additional Insured.
Award
The District reserves the right to accept any or all parts of a submitted proposal. All proposals shall be irrevocable for a period of sixty (60) days from the bid opening.
Work is to start as soon as Lakeview School District and the bidder can mutually agree upon a date.

Bid Due 
1. All sealed proposals must be submitted to Laura McFadden, Assistant Superintendent of Finance, Lakeview School District, 15 Arbor Street, Battle Creek, MI 49015, no later than 2:00 PM on Wednesday, July 22, 2026.  Any proposal received after that time will be returned unopened to the sender.  Proposals will be opened in the District’s Administration Office at 15 Arbor Street, Battle Creek, Michigan at 2:00 P.M. on Wednesday, July 22, 2026. All proposals will be opened at the day and time stated above.  All proposals will be read aloud. Persons submitting proposals may attend, and will receive a list of companies who have submitted bids.

Other required documents
Bids shall be accompanied by a sworn and notarized statement disclosing any familial relationship that exists between the owner or any employee of the bidder and any member of the board, intermediate school board, or board of directors or the superintendent of the school district, intermediate superintendent of the intermediate school district, or chief executive officer of the public school academy.  Additionally, bids shall be accompanied by an Iran Economic Sanctions Act Certification.  The District will not accept a bid that does not include this sworn and notarized disclosure statement and certification.























Lakeview School District Elementary Digital Sign Replacement Project
SECTION 2 – BID FORMS
Elementary Digital Monument Sign Replacement Project
Instructions
Complete all forms in this section. Failure to submit required documents may render the bid non-responsive.
Bid Proposal Form
	Bidder Name
	


	Address
	


	Primary Contact
	


	Phone
	


	Email
	


	Michigan Contractor License
	


	Federal EIN
	


	Authorized Signature
	




The undersigned agrees to furnish all labor, materials, equipment, permits, supervision, engineering, installation, programming, training, warranty service, and incidentals necessary to complete the project in accordance with the Contract Documents.
Base Bid Pricing Schedule
	School
	Base Bid
	Alternate
	Completion

	Minges Brook Elementary
	
$
	
$
	


	Prairieview Elementary
	
$
	
$
	


	Riverside Elementary
	
$
	
$
	


	Westlake Elementary
	
$
	
$
	

	TOTAL PROJECT
	
$
	
$
	



Unit Prices
	Description
	Unit Price

	Additional excavation
	
$

	Additional concrete
	
$

	Rock removal
	
$

	Electrical conduit
	
$

	Landscape restoration
	
$


Contractor Qualifications
Years in business: __________
Number of comparable digital sign projects completed: __________
Authorized manufacturer/dealer: Yes / No
Licensed to work in Michigan: Yes / No
24-hour emergency service available: Yes / No
Project References
	Owner
	Project
	Contact
	Phone

	

	
	
	

	

	
	
	

	

	
	
	

	

	
	
	

	

	
	
	


Subcontractors
	Trade
	Company
	Contact

	Electrical
	

	

	Concrete
	

	

	Masonry
	

	

	Excavation
	

	

	Other
	

	


Certifications Included
Non-Collusion Affidavit
Iran Economic Sanctions Certification
Familial Relationship Disclosure (PA 517)
Conflict of Interest Certification
W-9






















Lakeview School District Elementary Digital Sign Replacement Project
SECTION 3 – Division 01 General Requirements
01 10 00 Summary of Work
Contractor shall furnish all labor, supervision, materials, equipment, engineering, permits, demolition, foundations, electrical coordination, installation, testing, startup, training, and warranty necessary to provide a complete digital monument sign system at the four elementary schools.
01 11 00 Project Locations
Work includes Minges Brook 435 Lincoln Hill Drive, Prairieview 1675 Iroquois Ave., Riversid650 Riverside Dr. , and Westlake Elementary School 1184 S. 24th St, Battle Creek, MI 49015.
01 20 00 Contractor Responsibilities
Verify field dimensions; coordinate utilities; obtain permits; protect public; maintain clean site; provide qualified supervision; comply with codes.
01 31 00 Project Coordination
Coordinate work with District to minimize disruption. Work affecting traffic or entrances shall be scheduled with the Owner.
01 32 00 Construction Schedule
Submit baseline schedule within 10 days of Notice to Proceed. 
01 33 00 Submittals
Submit shop drawings, structural calculations sealed by a Michigan PE, product data, paint samples, brick samples, graphics, software information and warranty documentation before fabrication.
01 35 00 Safety
Contractor responsible for OSHA compliance, fencing, pedestrian protection, traffic control, and daily housekeeping.
01 50 00 Temporary Facilities
Provide temporary barricades, signage, erosion control, dumpsters, and protection of existing utilities and landscaping.
01 60 00 Product Requirements
All products shall be new and from a single manufacturer where practical. Equal products require prior approval.
01 73 00 Execution
Protect existing improvements; restore disturbed lawns, pavement and landscaping; remove debris daily.
01 77 00 Closeout
Provide as-built drawings, O&M manuals, warranty certificates, software credentials, and owner training before final payment.
01 78 36 Warranties
Minimum five-year comprehensive sign/display warranty including labor and software support unless otherwise approved by the District.
























Lakeview School District Elementary Digital Sign Replacement Project
SECTION 4 – Division 02 Existing Conditions & Demolition
02 41 13 Existing Conditions
Contractor shall visit all sites and verify existing monument signs, utilities, grades and access prior to bidding.
02 41 19 Demolition
Remove existing monument signs, foundations as required, poles, hardware, electrical components and dispose of materials in accordance with law.
02 41 20 Salvage
Items designated by the Owner shall be protected and turned over to the District. All other removed materials become Contractor property unless otherwise directed.
02 50 00 Site Preparation
Locate underground utilities through MISS DIG 811. Protect existing irrigation, sidewalks, pavement and landscaping.
02 61 00 Excavation
Excavate as required for engineered foundations. Unsuitable material shall be removed and replaced with compacted structural fill.
02 65 00 Restoration
Restore disturbed, mulch, pavement, and landscaping to original or better condition. Seed and mulch lawn areas.
Quality Assurance
Field verify dimensions before fabrication. Notify the Owner immediately of conflicts affecting installation.
Reference Documents
Technical drawings and sign specifications included in Attachment A govern the design intent for sign removal, locations, and replacement.






Lakeview School District Elementary Digital Sign Replacement Project
SECTION 5 – Division 03 Concrete
03 10 00 General
Provide all labor, materials, equipment, forms, reinforcing steel, concrete, anchor bolts, placement, finishing, curing, and testing necessary for complete sign foundations.
03 20 00 Reinforcement
Provide ASTM A615 Grade 60 reinforcing steel. Place and support reinforcement to maintain specified cover. Lap splices per structural engineering.
03 30 00 Cast-in-Place Concrete
Concrete shall have a minimum compressive strength of 4,000 psi at 28 days with air entrainment suitable for Michigan freeze/thaw conditions.
Foundations
Construct drilled pier footings, reinforced slab as shown on approved shop drawings, and engineered calculations. Verify dimensions in the field before excavation.
Anchor Bolts
Install galvanized anchor bolts using manufacturer templates. Verify alignment before concrete placement.
Concrete Placement
Do not place concrete on frozen ground. Protect fresh concrete from freezing and rapid drying.
Finish
Finish exposed concrete smooth unless concealed. Repair honeycombs and defects immediately.
Testing
District reserves the right to require concrete testing and inspection at Contractor expense if deficiencies are suspected.
Restoration
Restore all disturbed grades, lawns, mulch, and pavement after foundation work.




Lakeview School District Elementary Digital Sign Replacement Project
SECTION 6 – Division 05 Metals
05 10 00 Structural Steel
Provide structural steel members as required to support monument signs and electronic message centers. Fabrication shall comply with AISC standards.
Steel Tubes
Use minimum 3x3x3/16-inch structural steel tube supports or engineered equivalent meeting project loads.
Fabrication
All steel shall be shop fabricated, welded by certified welders, cleaned, primed, and protected from corrosion.
Galvanizing
Exterior steel exposed to weather shall be hot-dip galvanized or coated with an approved corrosion-resistant system.
Aluminum Cabinet
Provide extruded aluminum sign cabinet with welded construction, internal reinforcement, removable service panels, and factory finish.
Connections
Anchor, weld, and bolt all structural members in accordance with engineered shop drawings.
Engineering
Provide structural calculations signed and sealed by a licensed Michigan Professional Engineer verifying compliance with applicable wind loads.
Inspection
Owner reserves the right to inspect fabrication before shipment.
Warranty
Structural steel and aluminum fabrication shall carry a minimum five-year warranty against defects in materials and workmanship.




Lakeview School District Elementary Digital Sign Replacement Project
SECTION 7 – Division 10
Digital Monument Signs
This section establishes the minimum performance, material, fabrication, installation, software, and warranty requirements for the Elementary Digital Monument Sign Replacement Project. The drawings and site layouts provided by the District are incorporated by reference as Attachment A and establish the minimum design intent.
10 14 00.1 Scope
Provide complete turnkey digital monument signs including demolition, foundations, structural steel, aluminum cabinet, masonry base, internally illuminated cabinet, double-sided LED message center, electrical coordination, programming, startup, training, and warranty.
10 14 00.2 Acceptable Manufacturers
[bookmark: _GoBack]Manufacturers meeting or exceeding all specified dimensional, performance, software, warranty, and service requirements.
10 14 00.3 Sign Construction
Provide double-sided monument signs matching the design intent. Cabinet shall be welded extruded aluminum with removable access panels and internal LED illumination. Finish shall be factory-applied polyurethane suitable for exterior exposure.
10 14 00.4 Electronic Message Center
Provide full-color outdoor LED display with minimum 10 mm pixel pitch or approved equal. Display shall automatically adjust brightness, support scheduling, graphics, animation, emergency messaging, and remote diagnostics.
10 14 00.5 Software
Provide cloud-based content management software with unlimited District users, role-based permissions, browser-based access, content scheduling, preview mode, and automatic software updates during the warranty period. No recurring license fees during the base warranty.
10 14 00.6 Communications
Provide integrated cellular communications with modem, antennas, activation, testing, and configuration. Coordinate service with the District.
10 14 00.7 Electrical
Coordinate with the District's electrical contractor where applicable. Furnish internal disconnects, surge protection, power supplies, and all internal wiring required for a complete operating system.
10 14 00.8 Masonry Base
Construct masonry base to match Attachment A using thin brick veneer, aluminum cap, reinforced subframe, and concealed fasteners.
10 14 00.9 Shop Drawings
Submit complete shop drawings showing dimensions, foundations, structural calculations, colors, brick samples, electrical requirements, anchor bolt layout, cabinet details, and installation procedures. A Michigan Professional Engineer shall seal structural calculations.
10 14 00.10 Installation
Install signs plumb, level, and true. Verify all field dimensions and utility locations prior to excavation. Restore disturbed pavement, lawn, mulch, irrigation, and landscaping.
10 14 00.11 Commissioning
Perform complete operational testing of lighting, LED display, communications, software, and scheduling functions. Demonstrate successful operation before acceptance.
10 14 00.12 Training
Provide a minimum of four hours of onsite training for District staff and furnish electronic and printed operation manuals.
10 14 00.13 Warranty
Provide a comprehensive minimum five-year warranty covering LED display, cabinet, structural components, electronics, software, communications equipment, labor, and travel. Warranty response shall be within two business days for non-critical issues and same-day remote response when possible.
10 14 00.14 Spare Parts
Provide replacement fuses, touch-up paint, specialty tools (if required), and recommended spare electronic components.
10 14 00.15 Closeout
Submit warranties, as-built drawings, engineering certifications, software credentials, maintenance instructions, and final inspection documentation before final payment.

Performance Requirements
	Requirement
	Minimum

	Outdoor Display
	Full Color LED

	Viewing
	Day/Night Automatic Brightness

	Content
	Text, Graphics, Images, Scheduling

	Users
	Unlimited District Users

	Warranty
	5 Years

	Training
	4 Hours Onsite

	Engineering
	Michigan PE Sealed Calculations

	Reference Standard
	Attachment A Drawings and Specifications






Lakeview School District Elementary Digital Sign Replacement Project
SECTION 8 – Division 26 Electrical
26 05 00 General Requirements
Provide all electrical components required for a complete operational sign system. Coordinate with the District and utility provider where required.
26 05 19 Conductors and Wiring
Provide copper conductors, conduit, fittings, grounding, disconnects, surge protection, and wiring methods compliant with the current Michigan Electrical Code.
26 05 26 Grounding
Ground all metallic components and electrical equipment in accordance with NEC requirements.
26 05 33 Conduit
Install underground PVC conduit and above-grade rigid metallic conduit where exposed unless otherwise approved.
26 24 16 Panel Connections
Coordinate dedicated 120V circuits to each sign. Verify available capacity before beginning work.
26 27 26 Devices
Provide lockable disconnect switches, surge suppression, and weatherproof equipment.
26 56 00 Sign Electrical
Provide complete wiring for cabinet lighting, LED display, communications equipment, controllers, and power supplies.
Testing
Verify voltage, grounding, communication, brightness control, scheduling functions, and proper operation before acceptance.
Documentation
Provide wiring diagrams, as-built electrical drawings, equipment manuals, and maintenance recommendations.




Lakeview School District Elementary Digital Sign Replacement Project
SECTION 9 – Contract Documents
Owner-Contractor Agreement
The successful bidder shall execute the District's Agreement incorporating the Elementary Digital Sign Replacement Project, Drawings, Addenda, Bid Form, and Notice of Award.
Notice of Award
Issued by the District following Board approval.
Notice to Proceed
Establishes the official commencement date for contract time.
Certificates of Insurance
Evidence of required insurance must be submitted before work begins.
Final Completion
Submit closeout documents, warranties, as built, training documentation, and final lien waivers.
Warranty Certificate
Provide written warranty beginning on the date of final acceptance.

Required Closeout Documents
	Document
	Submitted

	As-Built Drawings
	

	Warranty Certificates
	

	Operation & Maintenance Manuals
	

	Training Record
	

	Software Credentials
	

	Final Waivers
	

	Final Inspection Report
	








Lakeview School District Elementary Digital Sign Replacement Project
SECTION 10 – Michigan Required Certifications & Bid Forms
Non-Collusion Affidavit
Bidder certifies proposal was independently prepared without collusion.
	Company
	

	Authorized Signature
	

	Printed Name
	

	Date
	



Conflict of Interest Certification
Bidder discloses any actual or potential conflicts of interest.
	Company
	

	Authorized Signature
	

	Printed Name
	

	Date
	



Certification Regarding Debarment
Bidder certifies it is not suspended or debarred from public contracting.
	Company
	

	Authorized Signature
	

	Printed Name
	

	Date
	



W-9
Successful bidder shall provide a completed IRS Form W-9 before payment processing.

Insurance Certification
Provide certificates meeting contract limits and naming Lakeview School District as additional insured.

Reference Certification
Provide at least three K-12 references for similar installations completed within the past five years. 


Familial Disclosure Affidavit

The undersigned, the owner or authorized officer of the below-named contractor (the “Contractor”), pursuant to the familial disclosure requirement provided in the Lakeview School District’s (the “School District”) Invitation to Bid for Elementary Data Cabling Demo and Install, hereby represents and warrants that, except as provided below, no familial relationships exist between the owner or any employee of the Contractor, and any member of the Board of Education of the School District or the Superintendent of the School District.  A list of the School District’s Board of Education Members and its Superintendent may be found at www.lakeviewspartans.org.

List any Familial Relationships:


Contractor:
							
____________________________________________________________________________
Print Name of Contractor
			

By:	______________________________________________________________________

Its:	______________________________________________________________________

Date:	______________________________________________________________________

State of ____________________________	)
) ss.
County of____	_______________________	)

This instrument was acknowledged before me on the _______ day of ________________________, 2026, 

by __________________________________________________________________________________________.

________________________________________________________________, Notary Public

_________________________________________ County, ___________________________

My Commission Expires:	____________________________________________________	

Acting in the County of:	____________________________________________________







Affidavit of Compliance - Iran Economic Sanctions Act
Michigan Public Act No. 517 of 2012

The undersigned, the owner or authorized officer of the below-named contractor (the “Contractor”), pursuant to the compliance certification requirement provided in the Lakeview School District’s (the “School District”) Invitation to Bid for Elementary Data Cabling Demo and Install (the “ITB”), hereby certifies, represents and warrants that the Contractor (including its officers, directors and employees) is not an “Iran linked business” within the meaning of the Iran Economic Sanctions Act, Michigan Public Act No, 517 of 2012 (the “Act”), and that in the event Contractor is awarded a contract a result of the aforementioned ITB, the Contractor will not become an “Iran linked business” at any time during the course of performing and services under the contract.

The Contractor further acknowledges that any person who is found to have submitted a false certification is responsible for a civil penalty of not more than $250,000.00 or two (2) times the amount of the contract or proposed contract for which the false certification was made, whichever is greater, the cost of the School District’s investigation, and reasonable attorney fees, in addition to the fine.  Moreover, any person who submitted a false certification shall be ineligible to bid on a request for proposal for three (3) years from the date that it is determined that the person has submitted the false certification.

CONTRACTOR:
							
__________________________________________________________	
Print Name of Contractor
							
By:	____________________________________________________	

Its:	____________________________________________________	
							
Date:	____________________________________________________	

STATE OF	___________________________________	)
)ss.
COUNTY OF	___________________________________	)

This instrument was acknowledged before me on the _________day of _________________________, 2026, 

by:  ____________________________________________________________________________________	

_________________________________________, Notary Public	

________________________________ County,	_________________

My Commission Expires:	___________________________________

Acting in the County of:	___________________________________




Lakeview School District Elementary Digital Sign Replacement Project
SECTION 11 – Appendices
Appendix A – Technical Drawings and Sign Specifications
Owner-furnished drawings establish the minimum design intent for dimensions, materials, site layouts, electrical coordination, foundation concepts, and appearance. Include the attached drawing package as Attachment A in the final bid manual.
Appendix B – School Locations
Lists the four project sites with addresses and owner contacts.
Appendix C – Bid Schedule
Final advertisement dates, pre-bid meeting, bid opening, award, and notice to proceed.
Appendix D – Insurance Requirements
Minimum insurance limits, endorsements, and certificate requirements.
Appendix E – Product Data
Successful bidder shall submit product data, shop drawings, structural calculations, color samples, brick samples, and software documentation.
Appendix F – Closeout Checklist
As-built drawings, warranties, O&M manuals, software credentials, training records, spare parts, and final waivers.




Appendix A – Technical Drawings and Sign Specifications
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PAINT: ALL ALUMINUM WILL BE DEGREASED, SANDED, PRIMED, & PAINTED WITH AKZO NOBEL ACRYLIC POLYURETHANE PAINT WITH SATIN FINISH CABINETS / SAND TEXTURE MASONRY CAP.
EMC: 3'-5" X 8'-3" WATCHFIRE 10MM (PIXEL MATRIX) EMC WITH ALUMINUM END PANELS PAINTED BLACK.

CLOUD-BASED SOFTWARE, LIFETIME 4G CELL MODEM COMMUNICATION, 5 YEAR PARTS/3 YEAR LABOR WARRANTY. INCLUDES NEW STEEL ANGLE MOUNTING FRAME.

INSTALLATION: ON NEW STEEL POST INSTALLED IN CONCRETE FOUNDATION. REMOVE & DISPOSE OF EXISTING SIGN.

NOTE: CUT OFF EXISTING STEEL POLE 6” BELOW GRADE & BACK FILL. NEW FOUNDATION TO BE SHIFTED OVER TO MISS EXISTING FOUNDATION AS NEEDED.
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