ADDENDUM 2
7/20/2026

RFQ 260000000373 DNR BOSTON WHALER 210 GUARDIAN – BRAND SPECIFIC

APPROVED ALTERNATE DNR SPECIFICATIONS
BID DUE DATE WAS EXTENDED TO JULY 31, 2026 AT 3:00 P.M. EST

DNR LAW ENFORCEMENT DIVISION PROVIDED SPECIFICATIONS TO INCLUDE SCOUT 220 XSF AS AN APPROVED ALTERNATE

BIDDERS WHO HAVE ALREADY SUBMITTED A PROPOSAL 
PLEASE REVIEW THE REVISED DNR SPECIFICATIONS


	GENERAL DNR SPECIFICATIONS

	21’ center console fiberglass hall

	T-top hardtop

	200hp outboard motor

	Trailer to transport the vessel

	Garmin 943XS

	Garmin GT12M Transducer

	Hydraulic steering

	Leaning post / Helm seating / w/ cooler

	Battery charger(house & engine bank)

	Raw water washdown w/ separate pump

	Bow bolsters & full bow cushion set

	Folding Transom Stern Seat

	console cover

	Galvanized Tandem axle trailer with swing tongue, Radial tires, Spare tire & disc brakes. 



PRE-APPROVED BRANDS / MODELS / SPECIFICATIONS
	SPECIFICATION 1

	Boston Whaler

	210 Guardian

	2026 or newer

	White with Black ID & Trim

	21 ft. 4 in.

	8 ft. 6 in.

	7

	UNSINKABLE HULL W/ COMMERCIAL FIBERGLASS

	SELF-BAILING HULL WITH SCUPPERS

	8" STAINLESS STEEL CLEATS (5)

	19" INTERIOR FREEBOARD

	HEAVY DUTY RUBRAIL

	BLACK IDENTIFICATION AND TRIM MARKINGS

	REVERSIBLE PILOT SEAT WITH LOCKING BACKREST AND STORAGE

	LOW PROFILE SS RAILS - BOW AND STERN

	STAINLESS STEEL BOW AND STERN EYES

	SWIM PLATFORM (FIBERGLASS) WITH GRAB RAIL AND LADDER

	DUAL BATTERY BOXES AND SWITCH

	FUEL CAPACITY: 66.5 GALLONS

	10-YEAR LIMITED HULL WARRANTY

	WHITE HULL - FULL (INTERIOR & EXTERIOR Included Included

	7 1 01050 BLACK GRAPHICS & T-TOP/HARDTOP FRAME

	RAW WATER WASH DOWN

	HELM AREA FLOOR PADDING (.75" Seadeck)

	COMMERCIAL & GOVERNMENT MODEL & OPTIONS

	HEAVY DUTY T-TOP W/ BLK CANVAS

	HD RUB STRAKES - VERTICAL ANGLE

	BATTERY PACKAGE (2 GR 27 AGM Batteries and 2 Fire Extinguishers)

	150 XL EFI 4-STROKE MERCURY ENGINE

	9" SIMRAD NSX ELECTRONICS / NAVIGATION 3-1 transom transducer

	WHELEN ION LED STROBE LIGHTS QNT 4 (switch activated) BLUE lights (only w/o H/T)

	WHELEN AMP & SIREN W/MIC (STROBE LTS separately) (only available w/o H/T) (not available with cooler)

	GALVANIZED TANDEM AXLE TRAILER WITH SWING TONGUE, RADIAL TIRES, SPARE TIRE & DISC BRAKES

	INLAND FREIGHT: (US & CANADA)

	REQUIRES MARINE LIFT OR LARGE FORKLIFT TO OFFLOAD FROM SEMI TRAILER *

	PRODUCTION AVAILABILITY: 150-180 days from receipt of purchase order

	PRODUCTION TIMELINE IS APPROXIMATELY 35 DAYS FROM START DATE

	PRODUCTION SLOT ESTABLISHED UPON RECEIPT OF PURCHASE ORDER OR AWARD

	SPECIFICATION 2

	SCOUT

	220 XSF

	2026 OR NEWER

	*SCOUT WHITE HULL (STANDARD)

	22 FT. 3.5IN.

	8FT.  6IN. 

	9

	SEA STAR HYDRAULIC STEERING UPGRADE (MUST ORDER W/ HP OVER 150)

	STANDARD LEANING POST (POWDER COATED HYBRID LEANING POST W/ IGLOO COOLER

	BATTERY CHARGER (HOUSE & ENGINE BANK)

	S.S. SPLIT BOW RAILS

	6” SPRING CLEATS

	8” PULL UP STERN CLEATS

	ON / OFF DUAL BATTERY SELECT SWITCH

	AFT PORT & STBD BOLSTERS

	BOW BOLSTERS & FULL BOW CUSHION SET

	SELF-BAILING COCKPIT

	DIGITAL GAUGES

	FUEL CAPACITY: 84 GALLONS

	POWDER COATED T-TOP HARDTOP W/ ELECTRONICS BOX AND INTEGRATED WINDSHIELD

	FWD SUN LOUNGE / COFFIN BOX W/ CUSHION

	PORT & STBD SWIM PLATFORMS W/ LADDER

	RAW WATER WASHDOWN W/ SEPARATE PUMP

	FOAM PAD ON SWIM PLATFORMS

	POWDER COATED ALUM. LEANING POST W/ BACKREST & 72QT IGLOO COOLER

	TRANSOM DOOR

	PREMIUM GEL-COAT

	NUV3 HULL

	Yamaha F200XD

	Garmin Display (1) 943XS

	Garmin GT12M Transducer

	GALVANIZED TANDEM AXLE TRAILER WITH SWING TONGUE, RADIAL TIRES, SPARE TIRE & DISC BRAKES

	PRODUCTION AVAILABILITY: ___________________________________________________

	PRODUCTION TIMELINE IS APPROXIMATELY ____ DAYS FROM START DATE

	



