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[bookmark: _Hlk53643277]Schedule A – Statement of Work
[bookmark: _Hlk205821848][bookmark: _Hlk205822275]Department of Natural Resources 
Law Enforcement Division
Boston Whaler 21 FT. Guardian Boat Package – per DNR Specifications
Brand Specific – Proposals offering alternate brands may not be considered for award.
Request for Quote No.  260000000373

REVISED 7/20/2026
MANDATORY DOCUMENT
Complete and attach to proposal in SIGMA VSS
This schedule identifies the anticipated requirements of any Contract resulting from this RFQ. The term “Contractor” in this document refers to a bidder responding to this RFQ, as well as the Contractor who is awarded the contract. The term “bidder” is used to identify where specific responses to the RFQ are required.  The Contractor must respond to each requirement or question and explain how it will fulfill each requirement. Attach any supplemental information and reference within your response.
[bookmark: _Hlk12451274][bookmark: _Hlk39820706]
SCOPE
The DNR is seeking bids for:
· ONE Boston Whaler 210 Guardian 21 Ft. boat package with Boston Whaler boat, outboard motor and boat trailer, per DNR specifications 
OR
· ONE approved comparable alternate Scout 220 XSF 22 Ft. boat package with Scout boat, outboard motor and boat trailer, per DNR specifications.     
The bidder must be the manufacturer or the authorized dealer / distributor of the brand proposed.  
Requirements
1. General Requirements
1.1. BOSTON WHALER 210 Guardian
1. Model 210 Guardian
2. Model Year 2026 or Newer
3. Boat Color Preferred: White with Black Identification and Trim Markings
4. Length: 21 ft. 4 in.
5. Beam Width:  8’ 6”
6. Maximum Persons: 7
7. Black T-Top / Hardtop Frame
8. Fuel Tank Size: 66.5 gallons
9. Hull Material – Unsinkable Hull W/ commercial fiberglass
10. Self-Baling hull with scuppers
11. 8” stainless steel cleats (5)
12. 19” interior freeboard
13. Heavy duty rub strakes – vertical angle
14. Reversible pilot seat with locking backrest and storage
15. Stainless steel bow and stern eyes
16. Low bow rail – stainless steel
17. Swim platform (fiberglass) with grab rail and ladder
18. 10-Year Hull Warranty
19. White Hull – full gelcoat (interior and exterior
20. 200 HP Maximum HP Capacity
21. Garmin 943XS
22. Garmin GT12M Transducer
23. Hydraulic steering
24. Leaning post / helm seating / w/cooler
25. Battery charger (house & engine bank)
26. Raw water washdown with separate pump
27. Bow bolsters & full bow cushion set
28. Folding transom stern seat
29. Console cover
30. WHELEN ION LED STROBE LIGHTS QNT 4 (switch activated) BLUE
31. WHELEN ION AMP & SIREN W/MIC (STROBE LTS separately)
32. Battery Package (2 GR 27 AGM Batteries and 2 fire extinguishers)
33. 9” Simrad NSX Electronic / Navigation 3-1 transom transducer
34. Helm area floor padding (.75” Seadeck)
35. Mercury 150 XL EFI 4-stroke engine or comparable 200 XL SeaPro V6
1. 2026 or Newer
2. Prop:  Standard Aluminum
3. Throttle / Shift:  Remote Mechanical
4. Starter:  Electric
5. Trim & Tilt:  Power Trim & Tilt
6. Rotation:  Standard
36. Galvanized Tandem Axle Trailer with Swing Tongue, radial tires, spare tire and disc brakes – correctly sized to fit Boston Whaler 210 Guardian
37. Price must include shipping, FOB Destination, 1732 West M32, Gaylord, MI  49735.

OR

1.2. SCOUT 220 XSF
1. Model 220 XSF
2. Model Year 2026 or newer
3. Boat Color Preferred:  *Scout White Hull (standard)
4. Length:  22 ft. 3.5in.
5. Beam Width:  8’ 6” 
6. Maximum Persons:  9
7. Sea Star Hydraulic Steering Upgrade (must order w/ HP over 150)
8. Standard Leaning Post (Powder Coated Hybrid Leaning Post w/ Igloo Cooler
9. Battery Charger (House & Engine Bank)
10. S.S. Split Bow Rails
11. 6” Spring Cleats
12. 8” Pull Up Stern Cleats
13. On / Off Dual Battery Select Switch
14. Aft Port & Starboard Bolsters
15. Bow Bolsters & Full Bow Cushion Set
16. Self-Bailing Cockpit
17. Digital Gauges
18. fuel capacity: 84 gallons
19. Powder Coated T-top Hardtop w/ Electronics Box and Integrated Windshield
20. Foward Sun Lounge / Coffin Box w/ Cushion
21. Port & Starboard Swim Platforms w/ Ladder
22. Raw Water Washdown w/ Separate Pump
23. Foam Pad on Swim Platforms
24. Powder Coated Alum. Leaning Post w/ Backrest & 72qt Igloo Cooler
25. Transom Door
26. Premium Gelcoat
27. NuV3 Hull
28. Garmin Display (1) 943XS
29. Garmin GT12M Transducer
30. Yamaha F200XD
1. 2026 or Newer
2. Prop:  Standard Aluminum
3. Throttle / Shift:  Remote Mechanical
4. Starter:  Electric
5. Trim & Tilt:  Power Trim & Tilt
6. Rotation:  Standard
31. GALVANIZED TANDEM AXLE TRAILER WITH SWING TONGUE, RADIAL TIRES, SPARE TIRE & DISC BRAKES – correctly sized to fit Scout 220 XSF
32. Price must include shipping, FOB Destination, 1732 West M32, Gaylord, MI  49735.

	[bookmark: _Hlk11243344][bookmark: _Hlk11942368]Bidder’s Response.  Bidder to check ONE box only, and identify exception(s)

	☐
	I have reviewed the above requirements and agree with no exception.

	☐
	I have reviewed the above requirement and have noted all exception(s) in column to the right.
	List all exception(s)

	Proposal is for:

	Boston Whaler 210 Guardian, per DNR Specifications:
	     ☐  YES     ☐  NO

	Scout 220 XSF, per DNR  Specifications:  
	     ☐  YES     ☐  NO



DELIVERY INFORMATION:
	INLAND FREIGHT – MANDATORY FOB DESTINATION
	     ☐  YES     ☐  NO

	REQUIRED MARINE LIFT OR LARGE FORKLIFT TO OFFLOAD FROM SEMI TRAILER
	     ☐  YES     ☐  NO

	PRODUCTION AVAILABILITY:  
	  _________ days from receipt of purchase order.

	PRODUCTION TIMELINE:
	  _________ days from start date.

	PRODUCTION SLOT ESTABLISHED:
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